# This file translates messages. It must be pairs of lines.
# The first line must say English: and then have the message from
# the program exactly. The second line must say Says: and then have
# any message you would like to actually see.

# Delete this file and run the program again to get all default messages.

English: 
Says:    

English: $_
Says:    $_

English: .)   MaxLineWidth n
Says:    .)   MaxLineWidth n

English: .)   MinLineWidth n
Says:    .)   MinLineWidth n

English: .)   SethLineWidth n
Says:    .)   SethLineWidth n

English: .)   SetlLineWidth n
Says:    .)   SetlLineWidth n

English: .)   TempLineWidth n
Says:    .)   TempLineWidth n

English: .)   XtrnLineWidth n
Says:    .)   XtrnLineWidth n

English: .) A range of bus addresses: E.g.: 1-8 or 8-1
Says:    .) A range of bus addresses: E.g.: 1-8 or 8-1

English: .) A single bus address. E.g.: 7
Says:    .) A single bus address. E.g.: 7

English: .) Comments start with ;
Says:    .) Comments start with ;

English: .) COMx
Says:    .) COMx

English: .) EMH n [C A W K V G], where n is the bus address of the EMH and one or more letters specify the EMH lines.
Says:    .) EMH n [C A W K V G], where n is the bus address of the EMH and one or more letters specify the EMH lines.

English: .) LineWidth n
Says:    .) LineWidth n

English: .) MaxLineColor  r g b
Says:    .) MaxLineColor  r g b

English: .) MinLineColor  r g b
Says:    .) MinLineColor  r g b

English: .) SethLineColor r g b
Says:    .) SethLineColor r g b

English: .) SetlLineColor r g b
Says:    .) SetlLineColor r g b

English: .) Simulate {On, Off}
Says:    .) Simulate {On, Off}

English: .) TempLineColor r g b
Says:    .) TempLineColor r g b

English: .) XtrnLineColor r g b
Says:    .) XtrnLineColor r g b

English: /RUNGUI     Start running the GUI interface
Says:    /RUNGUI     Start running the GUI interface

English: /RUNINDIA   Start running the India interface
Says:    /RUNINDIA   Start running the India interface

English: /STOP       Do not start running
Says:    /STOP       Do not start running

English: 1-8
Says:    1-8

English: ; automatically detect the regulators
Says:    ; automatically detect the regulators

English: ; Click Control / COM detect or
Says:    ; Click Control / COM detect or

English: ; Control / COM and Cell detect to
Says:    ; Control / COM and Cell detect to

English: ; Rudman Mark 3 Scanner
Says:    ; Rudman Mark 3 Scanner

English: ; See Help for file format definitions.
Says:    ; See Help for file format definitions.

English: ; This file is the GUI format file.
Says:    ; This file is the GUI format file.

English: COM13
Says:    COM13

English: Command line:
Says:    Command line:

English: Each bus address is displayed in the order specified. Duplicate bus addresses are illegal. Each EMH line is displayed in the order specified.
Says:    Each bus address is displayed in the order specified. Duplicate bus addresses are illegal. Each EMH line is displayed in the order specified.

English: Error trying to close the detected port
Says:    Error trying to close the detected port

English: Error trying to close the evil port
Says:    Error trying to close the evil port

English: Error trying to open the evil port
Says:    Error trying to open the evil port

English: Error trying to open the port
Says:    Error trying to open the port

English: Evil command
Says:    Evil command

English: Hit Enter to finish
Says:    Hit Enter to finish

English: Optionally give: filename evil_port
Says:    Optionally give: filename evil_port

English: Perl scanner version 2.13
Says:    Perl scanner version 2.13

English: Perl scanner version 2.14
Says:    Perl scanner version 2.14

English: Response
Says:    Response

English: Rudman Mark 3 Scanner
Says:    Rudman Mark 3 Scanner

English: Specify the default with a single dash, e.g.: scanner - COM6
Says:    Specify the default with a single dash, e.g.: scanner - COM6

English: The description file lines are used for Run GUI and Charger Test and are as follows:
Says:    The description file lines are used for Run GUI and Charger Test and are as follows:

English: The India format file lines may be simply COMx to switch to the given COM port, or a string of valid regulator commands separated by semicolon (;). If a command will not generate any output (e.g. 99h.) then prefix it with a exclamation point (!) otherwise --ERR-- will be displayed in the output.
Says:    The India format file lines may be simply COMx to switch to the given COM port, or a string of valid regulator commands separated by semicolon (;). If a command will not generate any output (e.g. 99h.) then prefix it with a exclamation point (!) otherwise --ERR-- will be displayed in the output.

English: The range of the graph is 0.2V beyond the actual recorded range of all bus addresses. An indicator line is present for both the low and high history for each bus address. The graph shows red up to the low history for any bus address that has been low. The graph shows blue (and resets the red) for any bus address that is currently high. The graph is green for any bus address currently between setlow and sethigh.
Says:    The range of the graph is 0.2V beyond the actual recorded range of all bus addresses. An indicator line is present for both the low and high history for each bus address. The graph shows red up to the low history for any bus address that has been low. The graph shows blue (and resets the red) for any bus address that is currently high. The graph is green for any bus address currently between setlow and sethigh.

English: This scanner uses an India format file or a description file to control the display of one or more regulators.
Says:    This scanner uses an India format file or a description file to control the display of one or more regulators.

English: Unknown simulation request
Says:    Unknown simulation request

English: Use Control / Run India or Control / Run GUI, depending on the format of your file.
Says:    Use Control / Run India or Control / Run GUI, depending on the format of your file.

